Cooledge FABRILum Specification Text

**Short (Fixture Schedule) – UL (N. America)**

A luminaire of dimensions a x b x c. Luminaire light output must be a minimum of xxxx delivered lumens with a minimum CRI = 9x, R9 > 65, 0.1% dimming level, and minimum operating frequency of 3000Hz. Acoustic performance to include a minimum Noise Reduction Coefficient (NRC) = xx; manufacturer to supply 3rd party acoustic test reports. Diffuser must be coated polyester fabric material, removable for maintenance without special tools, and have a minimum fire rating of ASTM E84 Class A. Luminaires must be UL Listed and carry a minimum warranty of 5 years.

*Values noted in blue are specific to the chosen model.*

**Short (Fixture Schedule) – CE**

A luminaire of dimensions a x b x c. Luminaire light output must be a minimum of xxxx delivered lumens with a minimum CRi = 9x, R9 > 65, 0.1% dimming level, and minimum operating frequency of 3000Hz. Acoustic performance to include a minimum Sound Absorption Average (SAA) = xx; manufacturer to supply 3rd party acoustic test reports. Diffuser must be removable for maintenance without special tools, and have a minimum fire rating of EN:3501-1 Class B. Luminaires must be CE Compliant and carry a minimum warranty of 5 years.

*Values noted in blue are specific to the chosen model.*